# V-Index
index: V

# Index

A B C D E F G H I K L M N O P Q R S T U V W X Y Z
All Classes and Interfaces | All Packages | Constant Field Values

## V

valueOf(String) - Static method in enum class swervelib.motors.SparkFlexSwerve.SparkMAX_slotIdx
  Returns the enum constant of this class with the specified name.
valueOf(String) - Static method in enum class swervelib.motors.SparkMaxSwerve.SparkMAX_slotIdx
  Returns the enum constant of this class with the specified name.
valueOf(String) - Static method in enum class swervelib.telemetry.Alert.AlertType
  Returns the enum constant of this class with the specified name.
valueOf(String) - Static method in enum class swervelib.telemetry.SwerveDriveTelemetry.TelemetryVerbosity
  Returns the enum constant of this class with the specified name.
values() - Static method in enum class swervelib.motors.SparkFlexSwerve.SparkMAX_slotIdx
  Returns an array containing the constants of this enum class, in the order they are declared.
values() - Static method in enum class swervelib.motors.SparkMaxSwerve.SparkMAX_slotIdx
  Returns an array containing the constants of this enum class, in the order they are declared.
values() - Static method in enum class swervelib.telemetry.Alert.AlertType
  Returns an array containing the constants of this enum class, in the order they are declared.
values() - Static method in enum class swervelib.telemetry.SwerveDriveTelemetry.TelemetryVerbosity
  Returns an array containing the constants of this enum class, in the order they are declared.
Velocity - Enum constant in enum class swervelib.motors.SparkFlexSwerve.SparkMAX_slotIdx
  Slot 2, used for velocity PID's.
Velocity - Enum constant in enum class swervelib.motors.SparkMaxSwerve.SparkMAX_slotIdx
  Slot 2, used for velocity PID's.
velocityPIDF - Variable in class swervelib.parser.SwerveModuleConfiguration
  PIDF configuration options for the drive motor closed-loop PID controller.
verbosity - Static variable in class swervelib.telemetry.SwerveDriveTelemetry
  The current telemetry verbosity level.
visionMeasurementStdDevs - Variable in class swervelib.SwerveDrive
  The standard deviation of the vision measurement, for best accuracy calculate the standard deviation at 2 or more points and fit a line to it and modify this using `SwerveDrive.addVisionMeasurement(Pose2d, double, Matrix)` with the calculated optimal standard deviation.

A B C D E F G H I K L M N O P Q R S T U V W X Y Z
All Classes and Interfaces | All Packages | Constant Field Values